{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":229,"n_cols":4,"rows_kept":229,"cut":false,"hidden":false,"merged":[[29,0,32,0],[29,1,32,1],[29,3,32,3],[0,0,2,0],[0,3,2,3],[3,0,3,3],[7,0,16,0],[7,1,16,1],[7,3,16,3],[17,0,20,0],[17,1,20,1],[17,3,20,3],[24,0,27,0],[24,3,27,3],[34,0,35,0],[34,1,35,1],[34,3,35,3],[41,0,42,0],[41,1,42,1],[41,3,42,3],[43,3,44,3],[49,0,49,3],[51,0,52,0],[51,1,52,1],[43,0,44,0],[43,1,44,1],[63,0,64,0],[63,1,64,1],[63,3,64,3],[67,0,67,3],[90,0,91,0],[90,2,91,2],[90,3,91,3],[68,0,69,0],[68,1,69,1],[68,2,69,2],[97,0,98,0],[97,1,98,1],[97,3,98,3],[142,0,143,0],[142,1,143,1],[142,3,143,3],[118,0,118,3],[119,0,123,0],[119,1,123,1],[124,0,128,0],[124,1,128,1],[124,3,128,3],[129,0,132,0],[129,1,132,1],[129,3,130,3],[131,3,132,3],[156,2,157,2],[158,0,159,0],[158,1,159,1],[158,2,159,2],[150,0,151,0],[150,1,151,1],[156,0,157,0],[156,1,157,1],[189,3,190,3],[162,0,163,0],[162,1,163,1],[162,3,163,3],[164,0,168,0],[164,1,168,1],[169,0,169,3],[174,0,175,0],[174,1,175,1],[174,2,175,2],[189,0,190,0],[189,1,190,1],[207,0,207,3],[196,0,197,0],[196,1,197,1],[196,2,197,2],[199,0,200,0],[199,3,200,3],[204,0,205,0],[204,1,205,1]],"flags":["formulas_cached_only"]}
["序号","测量仪器","测量仪器","规范名称及代号（含年号）"]
[null,"名称","类别/"]
[null,null,"典型型号"]
["一、长度"]
[1," 钢直尺"," 分度值：0.5mm","  JJG 1-1999 钢直尺检定规程"]
[2," 木直尺（折尺）"," 分度值：1mm"," JJG 2-1999 木直（折）尺检定规程"]
[3," 钢卷尺"," 分度值：0.5mm"," JJG 4-1999 钢卷尺检定规程"]
[4,"通用卡尺","游标卡尺","JJG30-2002 通用卡尺检定规程"]
[null,null,"分度值：0.01mm"]
[null,null,"电子数显卡尺"]
[null,null,"分辨率：0.01mm"]
[null,null,"带表卡尺"]
[null,null,"分度值：0.01mm"]
[null,null,"深度游标卡尺"]
[null,null,"分度值：0.01mm"]
[null,null,"电子数显深度卡尺"]
[null,null,"分辨率：0.01mm"]
[5,"指示表","百分表","JJG34-2008 指示表（百分表和千分表）检定规程"]
[null,null,"分度值：0.01mm"]
[null,null,"千分表"]
[null,null,"分度值：0.001mm"]
[6,"千分尺","分度值：0.01mm","JJG21-2008 千分尺检定规程"]
[7,"内径千分尺","分度值：0.01mm","JJG22-2003 内径千分尺检定规程"]
[8,"深度千分尺","分度值：0.01mm","JJG24-2003 深度千分尺检定规程"]
[9,"杠杆千分尺","杠杆千分尺：","JJG26-2001 杠杆千分尺、杠杆卡规检定规程"]
[null,"杠杆卡规","分度值：0.001mm"]
[null,null,"杠杆卡规："]
[null,null,"分度值：0.001mm"]
[10,"高度卡尺","分度值：0.01mm","JJG31-1999 高度卡尺检定规程"]
[11,"杠杆表","百分表：","JJG35-2006 杠杆表检定规程"]
[null,null,"分度值：0.01mm"]
[null,null,"千分表："]
[null,null,"分度值：0.001mm"]
[12,"量块","3等及以下","JJG 146-2003 量块检定规程"]
[13,"三针、针规","三针","JJF1207-2008 三针、针规校准规范"]
[null,null,"针规"]
[14,"塞尺","17片组","JJG62-2007 塞尺检定规程"]
[15,"百分表式卡规","分度值：0.01mm ","JJG109-2004 百分表式卡规检定规程"]
[16,"带表千分尺","分度值：0.001mm ","JJG427-2004 带表千分尺检定规程"]
[17,"深度百分表","分度值：0.01mm ","JJG830-2007 深度指示表检定规程"]
[18,"光滑极限量规","IT（6~11）","JJG343-1996 光滑极限量规检定规程"]
[19,"螺纹量规","螺纹塞规","JJG888-1995 圆柱螺纹量规检定规程"]
[null,null,"螺纹环规"]
[20,"内径表","百分表：分度值：0.01mm","JJF1102-2003 内径表校准规范"]
[null,null,"千分表：分度值：0.001mm"]
[21,"测量内尺寸千分尺","分度值：0.01mm","JJF1091-2002 测量内尺寸千分尺校准规范"]
[22,"光面环规","φ50mm","JJG894-1995 标准环规检定规程"]
[23,"工具显微镜","分度值：0.005mm","JJG56-2000 工具显微镜检定规程"]
[24,"投影仪","分度值：0.005mm","JJF 1093-2002 投影仪校准规范"]
["二、热工"]
[25,"数字温度计","数字型","JJG617-1996 数字温度指示调节仪检定规程"]
[26,"温度指示/调节/控制仪","动圈式","JJG186-1997 动圈式温度指示/指示位式调节仪表检定规程"]
[null,null,"数字式","JJG617-1996 数字温度指示调节仪检定规程"]
[27,"温度校准器","温度校准器","JJG617-1996 数字温度指示调节仪检定规程"]
[28,"测量记录仪"," 测量记录仪"," JJG 74-2005 工业过程测量记录仪检定规程"]
[29," 玻璃体温计"," 玻璃体温计"," JJG 111-2003 玻璃温度计检定规程"]
[30," 玻璃温度计"," 玻璃温度计"," JJG 130-2004 工作用玻璃液体温度计检定规程"]
[31," 温度巡回检测仪"," 温度巡回检测仪"," JJG 718-1991 温度巡回检测仪检定规程"]
[32," 温度变送器"," 温度变送器","JJG 829-1993 电动温度变送器检定规程"]
[33," 温度指示控制仪"," 温度指示控制仪"," JJG 874-1994 温度指示控制仪检定规程"]
[34," 模拟温度指示调节仪"," 模拟温度指示调节仪","JJG 951-2000 模拟式温度指示调节仪检定规程"]
[35,"温度试验设备","温度试验箱","JJF 1101-2003 环境试验设备温度、湿度校准规范"]
[36,"湿热试验设备","湿热试验箱","JJF 1101-2003 环境试验设备温度、湿度校准规范"]
[37,"高低温/低气压试验设备","高低温/低气压试","JJF 1101-2003 环境试验设备温度、湿度校准规范"]
[null,null,"验箱"]
[38,"数字采集系统","数字采集系统","JJF 1048-1995 数据采集系统校准规范"]
[39,"湿度传感器","湿度度传感器","JJF 1076-2001 湿度传感器校准规范"]
["三、力学"]
[40,"天平","Ⅰ级及以下","JJG 98-2006 机械天平检定规程"]
[null,null,null,"JJG 1036-2008 电子天平检定规程"]
[41,"数字指示秤","数字指示秤","JJG 539-1997 数字指示秤检定规程"]
[42," 模拟指示秤","模拟指示秤","JJG13-1997 模拟指示秤检定规程"]
[43," 非自行指示秤","非自行指示秤","JJG14-1997 非自行指示秤检定规程"]
[44," 架盘天平"," 架盘天平","JJG 156-2004 架盘天平检定规程"]
[45," 砝码"," 砝码","JJG 99-2006 砝码检定规程"]
[46," 测力仪"," 测力仪","JJG 144-1992 标准测力仪检定规程"]
[47,"称重传感器","称重传感器","JJG 669-2003 称重传感器检定规程"]
[48,"扭矩扳子","扭矩扳子","JJG 707-2003 扭矩扳子检定规程"]
[49," 测力杠杆","测力杠杆","JJG 808-1993 标准测力杠杆检定规程"]
[50,"扭矩测量仪","扭矩测量仪","JJG 995-2005 静态扭矩测量仪检定规程"]
[51,"金属洛氏硬度计","金属洛氏硬度计","JJG 112-2003 金属洛氏硬度计(A,B,C,D,E,F,G,H,K,N,T标尺)检定规程"]
[52," 金属维氏硬度计","金属维氏硬度计","JJG 151-2006 金属维氏硬度计检定规程"]
[53," A型邵氏硬度计","A型邵氏硬度计","JJG 304-2003 A型邵氏硬度计检定规程"]
[54," D型邵氏硬度计"," D型邵氏硬度计"," JJG 1039-2008 D型邵氏硬度计检定规程"]
[55,"扭力","扭力计","JJG 797-1992 扭矩扳子检定仪检定规程"]
[56," 推拉力计","推拉力计","JJG 455-2000 工作测力仪检定规程"]
[57,"万能材料试验机","万能材料试验机","JJG 139-1999 拉力、压力和万能试验机检定规程"]
[58," 非金属拉力、压力试验机"," 非金属拉力、压力试验机","JJG 157-1995 非金属拉力、压力和万能试验机"]
[59," 扭转试验机"," 扭转试验机","JJG 269-2006 扭转试验机检定规程"]
[60," 扭矩计"," 扭矩计","JJG 557-1988 标准扭矩计检定规程"]
[61,"  ","工作测振仪","JJG676-2000 工作测振仪检定规程"]
[null,"工作测振仪"]
[62,"电荷放大器","电荷放大器","JJG338-1997 电荷放大器检定规程"]
[63," 压电加速度计","压电加速度计","JJG233-2008 压电加速度计检定规程"]
[64," 速度传感器","速度传感器","JJG 134-2003 磁电式速度传感器检定规程"]
[65," 振动位移传感器","位移传感器","JJG 644-2003 振动位移传感器检定规程"]
[66," 轴承振动测量仪"," 轴承振动测量仪"," JJF 1185-2007 速度型滚动轴承振动测量仪校准规范"]
[67," 公害噪声振动计","噪声振动统计分析仪"," JJG 921-1996 公害噪声振动计检定规程"]
[null,null,"环境振动监测仪"]
[68," 基桩动态测量仪"," 基桩动态测量仪"," JJG 930-1998 基桩动态测量仪检定规程"]
[69,"动态信号分析仪","快速傅立叶变换型","JJG 834-2006 动态信号分析仪检定规程"]
[70,"电平记录仪","交流、直流","JJG(电子) 18002-1987 电平记录仪检定规程"]
[71,"转速测量仪","转速表","JJG105-2000 转速表检定规程"]
[72,"转速标准装置","转速标准装置","JJG 326-2006 转速标准装置检定规程"]
[73," 雷达测速仪"," 雷达测速仪"," JJG 528-2004 机动车雷达测速仪检定规程"]
[74," 机械振动试验台"," 机械振动试验台"," JJG189-1997 机械式振动试验台"]
[75," 电动振动试验台"," 电动振动试验台"," JJG190-1997 电动式振动试验台检定规程"]
[76," 液压振动试验台"," 液压振动试验台"," JJG638-1990 液压式振动试验台检定规程"]
[77," 数字式电动振动试验系统"," 数字式电动振动试验系统"," JJG948-1999 数字式电动振动试验系统检定规程"]
[78," 水平振动试验台","电动水平振动试验台"," JJG 1000-2005 电动水平振动试验台检定规程"]
[79," 标准振动台"," 中频标准振动台"," JJG 298-2005 中频标准振动台（比较法）检定规程"]
[80,"标准振动台","高频标准振动台","JJG 637-2006 高频标准振动台检定规程"]
[81," 水泥胶砂振动台"," 水泥胶砂振动台"," JJG 918-1996 水泥胶砂振动台检定规程"]
[82," 离心式稳态加速度试验台"," 离心机"," JJG 972-2002 离心式恒加速度试验机检定规程"]
[83,"冲击试验台","冲击试验台","JJG541-2005 落体式冲击试验台"]
[84," 摆锤式冲击试验机"," 摆锤式冲击试验机","JJG 145-1982 摆锤式冲击试验机鉴定规程"]
[85,"冲击测量仪","冲击测量仪","JJG 973-2002 冲击测量仪检定规程"]
[86,"碰撞试验台","碰撞试验台","JJG497-2000 碰撞试验台"]
["四、电学"]
[87,"数字多用表","直流数字电压表","JJG315-1983 直流数字电压表试行检定规程"]
[null,null,"交流数字电压表","JJG（航天）34-1999 交流数字电压表检定规程"]
[null,null,"直流数字电流表","JJG598-1989 直流数字电流表试行检定规程"]
[null,null,"交流数字电流表","JJG(航天)35-1999 交流数字电流表检定规程"]
[null,null,"电阻表","JJG724-1991 直流数字式欧姆表检定规程"]
[88,"模拟式多用表","直流电压表","JJG 124-2005 电流表、电压表、功率表及电阻表检定规程"]
[null,null,"交流电压表"]
[null,null,"直流电流表"]
[null,null,"交流电流表"]
[null,null,"电阻表"]
[89,"功率表","直流数字功率表","JJG780-1992 交流数字功率表检定规程"]
[null,null,"交流数字功率表"]
[null,null,"直流指针式功率表","JJG 124-2005 电流表、电压表、功率表及电阻表检定规程"]
[null,null,"交流指针式功率表"]
[90,"相位表","工频单相相位表","JJG 440-2008 工频单相相位表检定规程"]
[91,"直流电位差计","直流电位差计","JJG 123-2004 直流电位差计检定规程"]
[92,"电量变送器","电量变送器","JJG 126-1995 交流电量变换为直流电量电工测量变送器检定规程"]
[93,"电阻箱","微调电阻箱","JJG 486-1987 微调电阻箱试行检定规程"]
[94,"电阻分压箱","电阻分压箱","JJG 531-2003 直流电阻分压箱检定规程"]
[95,"模拟应变校准器","标准模拟应变校准器","JJG 533-1988 标准模拟应变校准器试行检定规程"]
[96,"电阻应变仪","电阻应变仪","JJG 623-2005 电阻应变仪检定规程"]
[97,"绝缘电阻表","绝缘电阻表","JJG 1005-2005 电子式绝缘电阻表检定规程"]
[98,"分压器","直流分压器","JJG 1007-2005 直流高压分压器检定规程"]
[99,"钳型表","直流钳型表","JJF1075-2001 钳形电流表校准规范"]
[null,null,"交流钳型表"]
[100,"数字电容表","数字电容表","JJG(电子)05006-1987 1620型电容测量装置试行检定规程"]
[101,"接地电阻表","接地电阻表","JJG 366-2004 接地电阻表检定规程"]
[102,"毫欧表","毫欧表","JJG 837-2003 直流低电阻表检定规程"]
[103,"直流电阻器","直流电阻器","JJG 166-1993 直流电阻器检定规程"]
[104,"直流电阻箱","直流电阻箱","JJG 982-2003 直流电阻箱检定规程"]
[105,"接地导通电阻测试仪","接地导通测试仪","JJG 984-2004 接地导通电阻测试仪检定规程"]
[106,"绝缘/高阻测量仪","绝缘电阻测量仪","JJG 622-1997 绝缘电阻表（兆欧表）检定规程"]
[null,null,"高阻计","JJG 690-2003 高绝缘电阻测量仪（高阻计）检定规程"]
[107,"直流电阻表","直流电阻表","JJG 724-1991 直流数字式欧姆表检定规程"]
[108,"直流电源","直流电源","JJG(航天) 6-1999 直流稳压电源检定规程"]
[109,"交流电源","交流电源(变频电源)","JJG(航天) 6-1999 直流稳压电源检定规程"]
[110,"电子负载","直流电子负载","JJF(电子) 30101-2007 直流电子负载校准规范"]
[111,"静电电压表","静电表","JJG 494-2005 高压静电电压表检定规程"]
[null,null,null,"JJG 315-83 直流数字电压表(试行)检定规程"]
[112,"分压器","分压器","JJG 496-1996"]
[null,null,null,"工频高压分压器检定规程"]
[113,"高压发生器","高压发生器","JJG 795-2004 耐电压测试仪试行检定规程"]
[114,"耐压测试仪","耐压测试仪","JJG 795-2004 耐电压测试仪试行检定规程"]
[115,"漏电流测量仪","直流泄漏电流测试仪(表)","JJG 843-2007 泄漏电流测量仪检定规程"]
[null,null,"交流泄漏电流测试仪(表)"]
[116,"多功能校准器","直流电压源","JJG 445-1986 直流标准电压源检定规程 "]
[null,null,"交流电压源","JJG 410-1994 精密交流电压校准源检定规程"]
[null,null,"直流电流源","JJG(航天) 38-1987 直流标准电流源检定规程"]
[null,null,"交流电流源","JJG(航天) 51-1999 交流标准电流源检定规程"]
[null,null,"电阻","JJG 166-1993 直流电阻器检定规程"]
["五、无线电"]
[117,"低频电压表","低频电压表","JJG250-1990 电子电压表检定规程"]
[118,"射频电压表","射频电压表","JJG308-1983 超高频毫伏表检定规程"]
[119,"超低频信号发生器","超低频信号发生器","JJG 64-1990 超低频信号发生器检定规程"]
[120,"函数信号发生器","函数信号发生器","JJG 840-1993 函数型号发生器检定规程"]
[121,"低频信号发生器","低频信号发生器","JJG602-1996"]
[null,null,null,"低频信号发生器检定规程"]
[122,"任意波形信号发生器","任意波形信号发生器","JJF 1152-2006 任意波发生器校准规范"]
[123,"高频信号发生器/合成信号生器","高频信号发生器/合成信号发生器","JJG173-2003 信号发生器检定规程"]
[124,"数字信号发生器","数字信号发生器","JJF 1174-2007 数字信号发生器校准规范"]
[125,"  脉冲信号发生器"," 脉冲信号发生器","JJG 490-2002脉冲信号发生器检定规程"]
[126,"正弦/噪声信号发生器","正弦/噪声信号发生器","JJG 607-2003 声频信号发生器检定规程"]
[127," 滤波器","1/1和1/3倍频程滤波器","JJG 449-2001 倍频程和1/3倍频程滤波器检定规程"]
[128,", 通用示波器","通用示波器","JJG262-1996 模拟示波器检定规程"]
[129,"取样示波器"," 取样示波器"," JJG491-1987 1GHz取样示波器检定规程"]
[130," 数字存储示波器"," 数字存储示波器"," JJF1057-1998 数字存储示波器"]
[131,"示波器高压探头","P6015A","JJF(电子) 30304-2008 示波器高压探头校准规范"]
[132,"示波器校准仪","通用型","JJG 278-2002 示波器校准仪检定规程"]
[133,"抖晃测量仪","抖晃测量仪","JJG 47-1990 抖晃仪检定规程"]
[134,"调制度","调制度测量仪/调制度分析仪","JJF 1111-2003 调制度测量仪校准规范"]
[135,"失真度测量仪","失真度测量仪","JJG251-1997 失真度测量仪检定规程"]
[null,null,"信纳表"]
[" 136"," 失真度校准仪","失真度校准仪","JJG 802-1993 失真度仪检定装置检定规程"]
[" 137","音频分析仪","音频分析仪","JJG(电子) 07006-1989  8903A音频分析仪试行检定规程"]
[138,"频谱分析仪","频谱分析仪","JJG501-2000 频谱分析仪检定规程"]
[139,"网络分析仪","网络分析仪","JJG(电子)07009-1991  HP-3577A型网络分析仪试行检定规程"]
[140,"EMI/EMC分析仪","EMI/EMC分析仪","JJF 1144-2006 电磁骚扰测量接收机校准规范"]
[141,"数字/模拟综合测试仪","数字/模拟综合测试仪","JJF 1065-2000 射频通信测试仪校准规范"]
[null,null,null,"JJF 1131-2005 TDMA-GSM数字移动通信综合测试仪校准规范"]
[142,"矢量信号分析仪","矢量信号分析仪","JJF 1128-2004 矢量信号分析仪校准规范"]
[143,"扫频仪/","扫频仪/","JJG(电子)07003 -1988 MSW-7124型调频调幅扫频仪试行检定规程"]
[null,"扫频信号发生器","扫频信号发生器"]
[144,"计数器/频率计","通用型","JJG349-2001 通用计数器检定规程"]
[145,"时间间隔测量仪","时间间隔测量仪、计时器","JJG 238-1995 数字式时间间隔测量仪试行检定规程"]
[146,"电子秒表","数字型","JJG 238-1995 数字式时间间隔测量仪试行检定规程"]
[147,"功率","功率计","JJG(航天)22-1987 436A型功率计检定规程"]
[null,null,"功率信号发生器","JJG 173-2003 信号发生器检定规程"]
[148,"衰减器","衰减器","JJG 387-2005 同轴电阻式衰减器检定规程"]
["六、声学"]
[149,"声级计","普通声级计","JJG 188-2002 声级计检定规程"]
[150,"声校准器","1000Hz","JJG 176-2005 声校准器检定规程"]
[151,"测试电容传声器","1000Hz","JJG 175-1998 测试电容传声器检定规程"]
[152,"声频功率放大器"," 声频功率放大器"," JJF 1200-2008 声频功率放大器校准规范"]
[153,"驻极体传声器测试仪"," 驻极体传声器测试仪"," JJF 1202-2008 驻极体传声器校准规范"]
[154,"扬声器功率寿命试验仪"," 扬声器功率寿命试验仪"," JJF 1203-2008 电声产品（扬声器类）功率寿命试验仪校准规范"]
[155,"传声器前置放大器","传声器前置放大器"," JJF 1137-2005 传声器前置放大器校准规范"]
[156,"测量放大器","测量放大器"," JJF 1157-2006 测量放大器校准规范"]
[157,"数字音频信号发生器","数字音频信号发生器"," JJG 994-2004 数字音频信号发生器检定规程"]
[157,"声频信号发生器","正弦/噪声信号发生器"," JJG 607-2003 声频信号发生器检定规程"]
[159,"猝发音信号源","猝发音信号源","JJG 199-1996 猝发音信号源检定规程"]
[160,"杂声计","杂声计","JJG 483-1987 杂声计检定规程"]
[161,"噪声剂量计","噪声剂量计","JJG 655-1990 噪声剂量计检定规程"]
[162,"噪声统计分析仪","噪声统计分析仪","JJG 778-2005 噪声统计分析仪检定规程"]
[163,"电话电声测试仪","电话电声测试仪","JJG 869-2002 电话电声测试仪检定规程"]
[164,"个人声暴露计","个人声暴露计","JJG 980-2003 个人声暴露计检定规程"]
[165,"声强测量仪","声强测量仪","JJG 992-2004 声强测量仪检定规程"]
[166,"建筑声学分析仪","建筑声学分析仪","JJF 1142-2006 建筑声学分析仪校准规范"]
[167,"驻极体传声器测试仪","驻极体传声器测试仪","JJF 1145-2006 驻极体传声器测试仪校准规范"]
[168,"音准仪","音准仪","JJF 1136-2005 音准仪校准规范"]
[169,"消声室","消声室","JJF 1147-2006 消声室和半消声室声学特性校准规范"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}